**6 M33.2 MARINE GENERATOR SET**

### Ratings

| **Duty** | **Hz** | **kWm** | **kWe** | **kVa** |
| --- | --- | --- | --- | --- |
| PRP | 50 | 205 | 472 | 590 |
| PRP | 60 | 224 | 520 | 650 |

### Engine Data

| **Cylinders** | **6-inline** |
| --- | --- |
| Bore & Stroke (mm) | 150x185 |
| Total Displacement (L) | 19.6 |
| Engine Rotation | Counterclockwise |
| Idle Speed (RPM) | 650 |

NO PDF ON SITE